|  |  |
| --- | --- |
| **CUSTOMER TO PROVIDE** | **BASTROP COUNTY REQUIREMENTS** |
| Driveway throat width | 12’ min – 24’ max |
| Turn Radius | Curbed Street: *Min. 5’ – Max 15’*  Uncurbed Street: *Min 10’ – Max 15’* |
| Distance from Property Line to start of Driveway | No part of the driveway or culvert may encroach on  any adjacent property within the County’s ROW |
| Driveway surface material | Must be all weather material to reduce tracking mud on county roadway & prevent damage to edge of pavement.  *Examples: Concrete, asphalt, chip seal, flex base, etc.* |
| Culvert material | CMP (Corrugated Metal Pipe) **or**  RCP (Reinforced Concrete Pipe) |
| Culvert diameter | Minimum 15”  *Arched (design) culvert acceptable to reduce culvert height* |
| Distance from edge of pavement to culvert | Used to determine if in clear zone |

